ITEM #: 40 GAL. PRESSURE TILTING SKILLET  
Quantity: One (1)  
Manufacturer: Rational   
Model No.: iVario Pro XL  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH, 96.0A; 3/4” HW, 3/4” CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide multifunctional cooking center with pressure cooking option.  
4. Provide one (1) 40-gallon pan.  
5. Provide integrated iVarioBoost energy management system, 85° to 480°F temperature range.  
6. Equip with with iZoneControl with up to (4) individually controlled heating zones.  
7. Equip with iCookingSuite intelligent cooking system.  
8. Equip with 6-point sensor core temperature probe.  
9. Provide AutoLift (baskets and arm required for use).  
10. Provide portioned water dispenser and retractable hand shower.  
11. Unit to be wifi enabled and equipped with ethernet interface.  
12. Unit to include Rational Chef Assistance Program.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.