ITEM #: AIR PURIFIER  
Quantity: One (1)  
Manufacturer: Franke  
Model No.: APS300  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 0.8A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be an Ultra Violet Purification System.  
4. Provide with heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
5. Unit shall have a refrigerated volume capacity up to 3600 cubic feet.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.