ITEM # : BACK BAR PASS-THRU REFRIGERATOR  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: PTS60  
Pertinent Data: Self Contained  
Utilities Req’d: 120V/1PH, 5.5 A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide four (4) 2-7/8” casters.  
4. Provide heavy duty cord and plug.  
5. Provide unit with 9 black vinyl-coated full-extension shelves (adjustable).  
6. Provide solid black vinyl clad doors with full length stainless steel handle.  
7. Provide four doors two hinged left and two hinged right.  
8. Coordinate installation under Item #, Back Bar Counter.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.