ITEM #: BASE AND DOME DRYING RACK  
Quantity: One (1)  
Manufacturer: Aladdin  
Model No.: SR100  
Pertinent Data: 100 Dome Capacity  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide durable, all-stainless-steel construction; unit frame includes 1” (2.54 cm) round stainless steel tubing. Cross supports are stainless steel “U” channel. The welded frame requires no assembly.  
4. Equip unit with 1” x 1.5” angle stainless steel shelf supports includes 1/4” high retainers which position wash racks on shelves.  
5. Provide removable, universal plastic wash racks include wire rack inserts that accommodate most domes and bases.  
6. Provide four (4) 5” swivel Poly-U/Poly-O casters with foot pedal brakes.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.