ITEM # : BEER DISPENSING TOWER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: 4006-4BPC  
Pertinent Data: ---  
Utilities Req'd: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide four (4) faucets on front.  
4. Provide faucet locks.  
5. Coordinate installation onto Item #, Draft Beer Cooler.  
6. Connect unit to Item #, Draft Beer Cooler.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.