ITEM # : BEER DISPENSING TOWER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: 4072-14PO-SS  
Pertinent Data: 1four (4) faucets  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide pure copper coolant lines and cold block.  
4. Provide insulated dispensing head and shank bushings.  
5. Provide four (4) faucets on front.  
6. Provide 308-40C beer faucet lock for 630 Series faucets.  
7. Coordinate installation onto Item #\_\_\_\_, Bar Top and Die.  
8. Connect unit to Item #\_\_\_\_, Beer System.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.