ITEM #: BEVERAGE COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing FS#   
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #1A, #2B, #4C, #5A, and #13.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide flanged feet, anchored to floor, on front legs only.  
5. Provide hinged cabinet doors with integrally formed full length door pull and intermediate shelves.  
6. Provide space on counter for Item #, Airpot Stand, Item #, Coffee Grinder, Item #, Coffee and Tea Brewer, Item #, Hot Water Dispenser, Item #, Double Sake Warmer, Item #, Coffee Grinder, Item #, Espresso Machine, and Item #, POS System.  
7. Provide cutouts and space under counter for Item #, Under Counter Freezer, Item #, Knock Box, Item #, Stainless Steel Trash Receptacle, Item #, Under Counter Refrigerator, Item #, Glass Filler Sink, Item #, Glass Rinser, Item #, Drop-In Ice Bin, Item #, Ice Cream Dipping Cabinet, Item #, Dipperwell, and Item #, Drop-In Hand Sink.  
8. Coordinate installation with Item #, Double Wall Shelf, and Item #, Liquor Storage Cabinet.  
9. Coordinate installation with Item #, Pass-Thru Window and Shelf.  
10. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.  
11. Provide shop drawings for approval prior to fabrication.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.