ITEM #: BLAST CHILLER  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: SBU 40 HT (965780040)  
Pertinent Data: Self-Contained  
Utilities Req’d: 400V/3PH, 4.6A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide Chilling capacity: 42kg from +90 degrees C to +3 degrees C in 90 minutes, Freeze capacity: 25kg from +90 degrees C to -18 degrees C in 240 minutes.  
4. Unit shall have stainless steel exterior.  
5. Equip unit to hold 1/1 GN pans (60mm spacing).  
6. Unit shall have automatic switching to storage mode after each cycle (+/- ).  
7. Equip unit with time circle starts automatically if user forgets to activate a process cycle.  
8. Provide a digital panel control board in a user friendly position and offering easy and rapid navigation.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.