ITEM #: BLENDER STATION WITH SINK & CABINET BASE  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSD12BLW  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 20.0A; 3/8” HW, 3/8” CW; 1-1/2” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide all stainless steel construction.  
3. Unit shall have stainless steel legs with removable stainless steel shrouding to limit access under the unit.  
4. Provide unit with 10-5/8” x 9-5/8” x 6” deep sink with hot and cold water, and gooseneck faucet.  
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.