ITEM # : BLENDER STATION WITH SINK  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TS12BLW  
Pertinent Data: ---  
Utilities Req’d: 3/8" HW, 3/8" CW; 1-1/2" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide all 20 gauge stainless steel construction.  
3. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.  
4. Provide unit with 9-1/4" x 11-1/4" x 6" deep sink with hot and cold water, and gooseneck faucet.   
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.