ITEM # : BOTTLE RAIL  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: SR-S36A  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide 36" long, locking speed rail.  
3. Coordinate installation onto Item #\_\_\_\_\_, Cocktail Station.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.