ITEM #: CENTRAL SANITATION SYSTEM  
Quantity: One (1)  
Manufacturer: Spray Master Technologies   
Model No.: SMT600REY (3005274)  
Pertinent Data: Central System  
Utilities Req’d: 208V/1PH, 9.0A, 3/4” CW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a model SMT 600REY Rack mounted master control panel with low voltage control cable.  
4. Provide 30-minute run timer, and water supply sensor switch.  
5. Provide 6’ water supply inlet hose.  
6. Provide stainless steel wall mounted brackets.  
7. Provide capability of two (2) chemicals to be injected by solenoids at the pump.  
8. Provide Item #, Portable Hose Reel, Hummer Jet Jr., trap shooter, wall and tile brush, and a wall bracket to hang accessories from.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.