ITEM #: CHEESEMELTER  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: ICMA-36  
Pertinent Data: ---  
Utilities Req’d: 3/4" Gas @ 40,000 BTUs; 5" WC  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacture’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide chrome plated heavy duty rack.  
4. Provide stainless steel front, sides, top and bottom.  
5. Coordinate installation over Item #, Hot Top with Oven.  
6. Provide control knobs that are durable cast aluminum with a chrome finish.  
7. Provide 48" flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.