ITEM #: CHOCOLATE MELTING MACHINE  
Quantity: One (1)  
Manufacturer: Hilliard’s  
Model No.: Little Dipper  
Pertinent Data:   
Utilities Req’d: 120V/1PH; 3.3A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 11.3kg tempering capacity.  
4. Provide unit to be constructed of stainless steel for sanitation as well as durability.  
5. Provide a digital readout.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.