ITEM # : COCKTAIL STATION  
Quantity: One (1)   
Manufacturer: Perlick  
Model No.: TS24IC  
Pertinent Data: ---  
Utilities Req’d: 1" IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide Tobin Ellis Signature Ice Chest, modular, 26"W, with approximately 50 lbs. ice capacity.  
3. Provide 6" high backsplash with 1" return.  
4. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.  
5. Provide ABS plastic top ledge, stainless steel top & sides, stainless steel interior, galvanized steel back & bottom.  
6. Provide stainless steel legs with adjustable thermoplastic feet.  
7. Provide ICC-C24,Tobin Ellis Signature Ice Chest Covers, 3-piece sliding assembly, 24"W, front & back, stainless steel (for TSC24 ice chests).  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.