ITEM #: COFFEE AND TEA BREWER  
Quantity: One (1)  
Manufacturer: Fetco  
Model No.: CBS1152V+  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH, 22.4A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide electrical configuration E115251.  
4. Equip unit with Extractor V+ Control Panel which will Control all brewing functions and diagnostic tools with user-friendly digital touch pad.  
5. Provide exclusive cascading spray dome.  
6. Unit shall produce 614, 8 oz. cups per hour.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.