ITEM # : COFFEE GRINDER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: 35600.0020  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 11A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide two (2) front loading 6 lbs. removable hoppers.  
4. Provide LCD alphanumeric display with three batch sizes per hopper.  
5. Provide precision burrs for consistent, commercial quality grind.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.