ITEM # : COFFEE GRINDER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: G9-2T DBC SST (33700.0000)  
Pertinent Data: ---  
Utilities Req’d: 230V/1PH, 1.32KW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide portion controlled for the right amount of coffee every time with 3 batch sizes per hopper.  
4. Equip unit with two hoppers each hold 6lb (2.72kg) of regular, decaf or specialty coffee beans.  
5. Unit shall be provided with a stainless steel finish.  
6. Must meet all applicable governmental, and local laws, rules, regulations, and codes.