ITEM # : COFFEE MAKER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: Sure Immersion 2-2-0 (44400.0100)  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 14.0A; 1/4" CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide two independent grinders with precision burrs for accurate grind profiles.  
4. Equip unit with beverage selections which include iced and hot options.  
5. Provide each recipe with programmable air-infusion and immersion control for the ideal result in the cup.  
6. Unit shall dispense fresh coffee in 5 portion sizes programmable from 6oz cup to 64oz carafe.  
7. Provide two tinted 3lb hoppers.  
8. Provide water filter 56000.0024 System, WEQ-10(1.5) 5L.  
9. Provide Sure Immersion installation package 24500.0782.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.