ITEM # : COLD BREW AND COFFEE DISPENSER  
Quantity: One (1)   
Manufacturer: Bunn  
Model No.: 51600.0022  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH, 6.0A; 3/8” CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit to serve two (2) flavors (both nitro), 4:1 - 12:1 product ratio.  
4. Provide LED lighted door with 11" x 6-1/2" changeable graphic panel.  
5. Unit to be able to serve two different coffees or teas as nitrogenated beverages using 1-gallon concentrate BIBs or refillable containers.  
6. Equip with BUNN gas infusion technology to produce up to 3 minutes of cascading micro-bubbles.  
7. Provide patented high intensity mixing chamber.  
8. Provide chrome-plated brass tap handles and black finish.  
9. Provide with 8-pound ice bank, automatic water bath fill, and refrigerated product cabinet.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.