ITEM #: CONTROL CENTER  
Quantity: One (1)  
Manufacturer: Aerowerks  
Model No.: Custom Design  
Pertinent Data: See Plans, Drawing  
Utilities Req’d: 208V/3PH; 4.7A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be an integral part of Item #, Soiled Rack Transport Conveyor.  
4. Provide unit with a stainless steel water-resistant cabinet.  
5. Unit shall control on/off and speed of Item #, Soiled Rack Transport Conveyor.  
6. Provide remotely located start/stop station with magnetic system that allows rollers to stop, but chain to continue moving when racks are accumulated on conveyor.  
7. Provide shop drawings for approval prior to fabrication.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.