ITEM #: DOUBLE DEEP KEG RACK  
Quantity: Four (4)  
Manufacturer: New Age  
Model No.: 51171  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide framework for the keg shelves, constructed out of 1-1/2@ x 2-3/4" x .070" wall tubing.  
4. Provide keg shelf laterals constructed out of 1-1/2@ x 2-11/16" x .15" wall channel.  
5. Provide posts that are constructed out of 1-5/16" Diameter pipe.  
6. Provide 12 Keg Capacity.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.