ITEM #: DOUBLE OVERSHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #29, and #30.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Coordinate installation of Item #, P.O.S. Printer.  
5. Ensure supports of Double Overshelf are attached to the frame of Item #, Chef’s Counter for stability.  
6. Provide shop drawings for approval prior to fabrication.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.