ITEM #: DOUGH DIVIDER/ROUNDER  
Quantity: One (1)  
Manufacturer: Gemini KB Systems  
Model No.: GBEDR  
Pertinent Data: Automatic  
Utilities Req’d: 208V/3PH; 4.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with electronic control panel.  
4. Provide automatic cycle of dividing and rounding.  
5. Unit shall be equipped with programmable pressing and rounding times.  
6. Equip unit with press only, divide only, and cleaning positions.  
7. Provide cast iron foot on wheels.  
8. Provide stainless steel dividing disc.  
9. Equip unit with interchangeable dividing disc.  
10. Unit shall be equipped with coated anodized aluminum dividing disc.  
11. Provide a forward tilting system which provides easier access for cleaning the dividing disc.  
12. Unit shall have two handed operation and cleaning position.  
13. Equip the unit with the following:  
 a. 14 Part Disc for 4.6oz to 8.8oz weight range.  
 b. 30 Part Disc for 1.4oz grams to 4.6oz weight range.  
 c. 36 Part Disc for 1.0oz to 4.0oz weight range.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.