ITEM # : DRAINBOARD  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: SC-18  
Pertinent Data: ---  
Utilities Req ‘d: 1" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer ‘s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be provided with 1-5/8" OD tubular stainless steel legs with 1" adjustable thermoplastic feet.  
3. Unit shall be constructed of embossed stainless steel drainboard.  
4. Provide unit with adjustable stainless steel shelf.   
5. Provide left hinged door.  
6. Provide shop drawings for approval prior to fabrication.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.