ITEM #: DRIP TRAY  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: 5020  
Pertinent Data: ---  
Utilities Req’d: 1/2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a stainless-steel drip pan.  
4. Coordinate installation of Item #\_\_\_\_, Dispensing Tower.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.