ITEM # : DRIP TROUGH  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: C18645A-GRC  
Pertinent Data: ---  
 Utilities Req’d: 1/2" CW; 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a stainless steel erip pan.  
4. Equip unit with a glass rinser of 4-3/8@ Diameter Heavy Gauge Stainless Steel Glass Rack, NSF Listed Stainless Steel Rinser.  
5. Coordinate installation onto Item #\_\_\_, Preparation/Back Counter with Sink.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.