ITEM # : DRIP TROUGH  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: C18750-21-GRC  
Pertinent Data: ---  
Utilities Req’d:

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be constructed of all stainless steel.  
4. Provide the glass rinser with at 4.37” (111mm) diameter heavy gauge stainless steel glass rack NSF listed stainless steel rinser.  
5. Coordinate installation into Item #\_\_\_\_, Back Bar Top and with Item #\_\_\_\_, Beer Dispensing Tower.  
6. Must meet all applicable governmental, and local laws, rules, regulations, and codes.