ITEM #: DROP-IN HAND SINK WITH SOAP & TOWEL DISPENSER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS\_\_\_, Drop-In  
Utilities Req’d: 1/2” CW, 1/2” HW, 1-1/2” DW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FS\_\_.2, Detail #24.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide with gooseneck faucet.  
5. Provide with c fold towel dispenser.  
6. Provide unit with p trap and tail piece.  
7. Provide unit with wrist blade.  
8. Unit must be cleanly continuously fully welded into place and ground smooth so that there are no cutting spots.  
9. Coordinate installation into Item #\_\_\_\_\_\_\_\_\_, as shown on drawings.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.