ITEM #: ENCLOSED FOOD TRANSPORT CART  
Quantity: One (1)  
Manufacturer: FWE  
Model No.: ETC-UA-13INS  
Pertinent Data: ---  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with four (4) 203mm diameter road worthy balloon, swivel, tires.  
4. Provide unit with 13 pair of tray/pan slides  
5. Provide unit with flush-mounted, stainless steel insulated door.  
6. Equip the unit with a padlocking transport latch.  
7. Provide heavy-duty tubular stainless steel push handles.  
8. Provide a cold plate cartridge.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.