ITEM # : ESPRESSO MACHINE  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: BW3-CTS (43500.0010)  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 30.0A; 3/8” CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be two-step model (automatic espresso + steam wand) with hot water dispense.  
3. Equip with an Intellisteam® wand automatically steams to proper milk temperature, no need to monitor with a thermometer  
4. Unit shall steam 1L of milk in under one minute.  
5. Provide two hoppers which allow for your choice of fresh espresso beans.  
6. Equip with easy-to-use touch screen with beautiful graphics which guides the operator.  
7. Unit shall have hopper capacity of 3.3lb (1.5kg).  
8. Equip the dispense spout to adjust from 3" to 6.8”.  
9. Equip the unit with a heated stainless steel brew chamber.  
10. Provide a heavy duty grinder.  
11. Provide a simple cleaning process with reminder and lockout.  
12. Equip unit with a built-in troubleshooting menu.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.