ITEM # : ESPRESSO MACHINE  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: BW4C CTM P-RS Superautomatic Espresso (55300.0002)  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 13.2A; 1/4" CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit to have capacity for 150 cups/day performance.  
4. Provide with a 4.4lb (2kg) chocolate powder system for mocha and hot chocolate beverages  
5. Unit to produce hot and cold foamed milk.  
6. Equip with two 2.2lb (1.0kg) bean hoppers with two grinders for fresh espresso beans.  
7. Provide an integrated single-milk refrigerator that holds up to 4L of milk.  
8. Equip with an easy-to-use touch screen with graphics to guide the operator.  
9. Provide with simple, screen-prompted cleaning process with reminder and lockout (daily cleaning for espresso and milk, weekly cleaning for powder).  
10. Provide an adjustable height product dispense spout (3.3" to 6.9").  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes