ITEM #: ESPRESSO MACHINE  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: Sure Tamp Steam (43400.0036)  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 20.4A; 1/4” CW; 5/8” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide two (2) hoppers.  
4. Equip unit with a dispense spout which accommodates cups up to 20oz.  
5. Unit shall maintain constant and consistent tamping pressure throughout the shot cycle.  
6. Provide BUNNlink7 machine to machine monitoring system.  
7. Equip unit with Intellisteam7 wand automatically steams to proper milk temperature no need to monitor with a thermometer.  
8. Coordinate installation onto Item #, Room Service Setup Counter with Sink.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.