ITEM #64: EVAPORATOR COIL  
Quantity: One (1)  
Manufacturer: RDT  
Model No.: BEL0095  
Pertinent Data: See Plans Drawing #FS\_\_\_, Connect to Building Emergency Power.  
Utilities Req'd: 120V/1PH, 1.8A; 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Evaporator shall be located where shown on drawings and interconnected to Item #\_\_\_, Refrigeration Rack.  
3. KEC to coordinate installation with General Contractor, and Electrical Contractor. Indirect waste to be terminated with a “P” trap.  
4. Provide shop drawings for approval prior to installations.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.