ITEM #: FLOOR TROUGH AND GRATE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FSX.X, Detail #3   
Utilities Req'd: 2” drain recessed 4”

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard Fabrication #FSX,X, Detail #3.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. All stainless steel construction.  
5. Provide perforated stainless steel grating.  
6. Provide shop drawings for approval prior to fabrication.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.