ITEM #: FOOD WARMER  
Quantity: One (1)  
Manufacturer: BSI  
Model No.: 490  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 9.2A (Depends on length)  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide infinite controls and remote-control enclosure.  
3. Provide an aluminum housing.  
4. Provide infrared heating element shall be tubular metal sheathed.  
5. Coordinate installation on Item #, Sneeze Guard.  
6. Verify finish color with the Architect and or Interior Designer.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.