ITEM #: GLASS RACK SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per plans, details, and the following:  
1. Standard Fabrication Drawing #FS?.? Detail #??.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide unit to be 18-gauge 304 stainless steel with #4 finish, bracket shall be 14-gauge 304 stainless steel.   
5. Coordinate installation above Item #, Soiled Dish Table.   
6. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.   
7. Provide shop drawings for approval prior to fabrication.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.