ITEM #: GLASS WASHING BRUSH  
Quantity: One (1)  
Manufacturer: Bar Maid  
Model No.: SS-100  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 10.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide the compact ASS@ series submersible glass washer.  
4. Provide optional accessory brushes.  
5. Coordinate installation into Item #, Three Compartment Sink.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.