ITEM #: GRAB-N-GO MERCHANDISER  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: FLM-54  
Pertinent Data: Double Section, Self-Contained  
Utilities Req’d: 120V/1PH; 6.3A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide black powder coated door, front and sides on the exterior, and white aluminum sides, wall and back on the interior.  
3. Provide heavy-duty cord and plug. Coordinate NEMA configuration with the Electrical Contractor.  
4. Provide two (2) full-height glass door, hinged left as shown on plans.  
5. Provide door locks.  
6. Provide illuminated sign decals on each door. Verify decals with the Interior Designer.  
7. Provide four (4) additional shelves.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.