ITEM #: HAND SINK WITH SOAP AND TOWEL DISPENSER  
Quantity: One (1)  
Manufacturer: IMC/TEDDY  
Model No.: WSSEC  
Pertinent Data: ---  
Utilities Req’d: 1/2” CW, 1/2” HW,1-1/2” DW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with handsfree automatic electronic faucet, battery powered models.  
3. Provide with correctional towel dispenser for 300 multifold towels.  
4. Provide unit with p trap.  
5. Provide battery-operated faucet.  
6. Provide 6 Volt battery to operate electronic sensor.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.