ITEM #: HAND SINK  
Quantity: One (1)  
Manufacturer: Eagle  
Model No.: HSA-10-FL  
Pertinent Data: ---  
Utilities Req’d: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit to be type 304 stainless steel, all-welded with deep-drawn positive drain sink bowl.  
3. Equip with inverted “V” edge to prevent spillage.  
4. Provide polymer lever drain.  
5. Provide unit with splash mounted gooseneck faucet.   
6. Soap and Towel Dispensers shall be by Vendor.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.