ITEM # : HAND SINK  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSD12HSN  
Pertinent Data: With Dispenser for folded paper towels  
Utilities Req’d: 3/8" HW, 3/8" CW; 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.   
3. Provide with towel and liquid soap dispenser.   
4. Provide unit with splash guards which shall be 12" high on sides and shall be mounted using stainless steel screws.  
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.