ITEM #: HOSE REEL CONTROL CABINET  
Quantity: One (1)  
Manufacturer: Fisher  
Model No.: 1801  
Pertinent Data: Stainless Housing  
Utilities Req’d: 15mm CW, 15mm HW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Install unit in location as shown on plans.  
3. Recess the Hose Reel Control Cabinet, see drawing #FS Detail #9.  
4. Interconnect to Item #, Hose Reel.  
5. Provide shop drawings for approval prior to installation.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.