ITEM #: HOSE REEL  
Quantity: One (1)  
Manufacturer: Fisher  
Model No.: 32026  
Utilities Req’d: 1/2” CW, 1/2” HW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Install unit in location as shown on plans.  
3. Unit shall be ceiling mounted see drawing #FS Detail #10.  
4. Connect the unit to Item #, Hose Reel Control Panel, see drawing #FS Detail #9.  
5. Provide with 30’ long hose.  
6. Provide shop drawings for approval prior to installation.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.