ITEM #: HOSE REEL  
Quantity: One (1)  
Manufacturer: Fisher  
Model No.: 75222  
Pertinent Data: See Plans Drawing #FS\_.1, Detail #6  
Utilities Req’d: 1/2" CW (From #\_\_\_)

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Install unit in location as shown on plans.  
3. Unit shall be ceiling mounted see drawing FS\_\_\_.1, Detail #6.  
4. Connect the unit to Item #57, Hose Reel Control Panel. See Drawing FS\_\_\_.1, Detail #7.  
5. Provide with 30' long hose.  
6. Provide shop drawings for approval prior to installation.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.