ITEM #: HOSE STATION CABINET  
Quantity: One (1)  
Manufacturer: Strahman  
Model No.: M750TG  
Pertinent Data: Recessed Wall Mounted, See Plans, Drawing #FS Detail #5  
Utilities Req’d: 3/4” CW, 3/4” HW, 1/2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation where shown on drawing.  
3. Provide unit with CE1000 stainless steel cabinet that shall house the unit.  
4. Cabinet shall be provided with drain in bottom of cabinet.  
5. Provide S75 hose assembly with a 50’ long white hose and a spray gun.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.