ITEM #: ICE AND WATER DISPENSER  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: DCM-300BAH-OS  
Pertinent Data: Self Contained, Air Cooled  
Utilities Req’d: 120V/1PH; 10.3A; 1/2” CW; 3/4” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide stainless steel bin and exterior, protected with H‐GUARD Plus Antimicrobial Agent.  
4. Unit shall be equipped with 40 lb. storage capacity.  
5. Equip unit with LED sensor operation.  
6. Coordinate with Plumbing Contractor on the connection between Ice And Water Dispenser and Item #\_\_\_, Water Filtration System.  
7. Coordinate installation onto Item #\_\_\_\_\_\_\_\_\_  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.