ITEM #: ICE AND WATER DISPENSER  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: HID450 A-6  
Pertinent Data: Self Contained, Air Cooled  
Utilities Req’d: 208V/1PH; 3.8A; 3/8” CW; 3/4” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide durable stainless steel evaporator and exterior panels.  
4. Unit shall be equipped with antimicrobial AquaArmor with AgIONJ is molded into key components.  
5. Equip unit with intuitive LED diagnostic lights reduce service time. Unit specific QR code for quick access to service manuals and warranty history.  
6. Coordinate installation onto Item #\_\_\_\_\_,Beverage and Condiment Counter.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.