ITEM #: ICE BIN  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: B-140SA  
Pertinent Data: 254 Pounds Capacity  
Utilities Req’d: 1” IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide stainless-steel front and sides, galvanized rear, and ABS plastic, light-weight, insulated door, for ease of handling and comfortable access to ice.  
4. Blue polyethylene bin liner with rounded corners allows for faster collection of ice.  
5. Provide back-panel drain connection.  
6. Coordinate installation of Item #\_\_\_, Ice Machine, on top of unit.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.