ITEM # : ICE CREAM DIPPING CABINET  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: 8000A  
Pertinent Data: Self Contained  
Utilities Req’d: 120V/1PH; 0.8A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a 20 gauge stainless steel top and removable hinged door lid with locking lid option.  
4. Unit shall have a 3 gallon capacity.  
5. Coordinate installation into Item #\_\_\_\_, Serving Counter.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.